Par Statistics
Total Non-vccgnd Signals= 162
Total Non-vccgnd Design Pins= 308
Total Non-vccgnd Conns= 308
Total Non-vccgnd Timing Constrained Conns= 293
Phase 1 CPU= 4.9 sec
Phase 2 CPU= 5.0 sec
Phase 3 CPU= 5.2 sec
Phase 4 CPU= 5.7 sec
Phase 5 CPU= 5.9 sec
Phase 6 CPU= 5.9 sec
Phase 7 CPU= 5.9 sec
Phase 8 CPU= 5.9 sec
Phase 9 CPU= 5.9 sec
Phase 10 CPU= 5.9 sec
AvgWirelenPerPin Fanout 1= 1.0
AvgWirelenPerPin Fanout 2= 1.0
AvgWirelenPerPin Fanout 3= 3.3
AvgWirelenPerPin Fanout 4= 1.0
AvgWirelenPerPin Fanout 10= 0.0
AvgWirelenPerPin Fanout 50= 3.2
AvgWirelenPerPin Fanout 100= 0.0
AvgWirelenPerPin Fanout 500= 0.0
AvgWirelenPerPin Fanout 5000= 0.0
AvgWirelenPerPin Fanout 20000= 0.0
AvgWirelenPerPin Fanout 50000= 0.0
AvgWirelenPerPin Fanout 100000= 0.0
IRR Gamma= 1.0242