Par Statistics
Total Non-vccgnd Signals= 619
Total Non-vccgnd Design Pins= 1634
Total Non-vccgnd Conns= 1634
Total Non-vccgnd Timing Constrained Conns= 1350
Phase 1 CPU= 4.8 sec
Phase 2 CPU= 5.3 sec
Phase 3 CPU= 6.6 sec
Phase 4 CPU= 7.1 sec
Phase 5 CPU= 8.5 sec
Phase 6 CPU= 8.5 sec
Phase 7 CPU= 8.5 sec
Phase 8 CPU= 8.5 sec
Phase 9 CPU= 8.6 sec
Phase 10 CPU= 8.7 sec
AvgWirelenPerPin Fanout 1= 3.0
AvgWirelenPerPin Fanout 2= 0.5
AvgWirelenPerPin Fanout 3= 2.3
AvgWirelenPerPin Fanout 4= 2.3
AvgWirelenPerPin Fanout 10= 2.4
AvgWirelenPerPin Fanout 50= 1.7
AvgWirelenPerPin Fanout 100= 9.6
AvgWirelenPerPin Fanout 500= 0.0
AvgWirelenPerPin Fanout 5000= 0.0
AvgWirelenPerPin Fanout 20000= 0.0
AvgWirelenPerPin Fanout 50000= 0.0
AvgWirelenPerPin Fanout 100000= 0.0
IRR Gamma= 1.1502