<?xml version="1.0" encoding="UTF-8"?>
<!-- IMPORTANT: This is an internal file that has been generated
     by the Xilinx ISE software.  Any direct editing or
     changes made to this file may result in unpredictable
     behavior or data corruption.  It is strongly advised that
     users do not edit the contents of this file. -->
<messages>
<msg type="warning" file="HDLCompiler" num="1127" delta="old" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\ipcore_dir\clk_pll.v" Line 126: Assignment to <arg fmt="%s" index="1">clkout3_unused</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="old" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\ipcore_dir\clk_pll.v" Line 127: Assignment to <arg fmt="%s" index="1">clkout4_unused</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="old" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\ipcore_dir\clk_pll.v" Line 128: Assignment to <arg fmt="%s" index="1">clkout5_unused</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="old" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\top.v" Line 57: Assignment to <arg fmt="%s" index="1">clk5m12</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="413" delta="old" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\top.v" Line 65: Result of <arg fmt="%d" index="1">5</arg>-bit expression is truncated to fit in <arg fmt="%d" index="2">4</arg>-bit target.
</msg>

<msg type="warning" file="HDLCompiler" num="413" delta="old" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\top.v" Line 73: Result of <arg fmt="%d" index="1">8</arg>-bit expression is truncated to fit in <arg fmt="%d" index="2">7</arg>-bit target.
</msg>

<msg type="warning" file="HDLCompiler" num="413" delta="old" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\top.v" Line 82: Result of <arg fmt="%d" index="1">4</arg>-bit expression is truncated to fit in <arg fmt="%d" index="2">3</arg>-bit target.
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="old" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\ir.v" Line 130: Assignment to <arg fmt="%s" index="1">T_Value</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="old" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\vga.v" Line 109: Assignment to <arg fmt="%s" index="1">PIX</arg> ignored, since the identifier is never used
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\top.v</arg>&quot; line <arg fmt="%s" index="2">52</arg>: Output port &lt;<arg fmt="%s" index="3">CLK_OUT3</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">pll_inst</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\top.v</arg>&quot; line <arg fmt="%s" index="2">52</arg>: Output port &lt;<arg fmt="%s" index="3">LOCKED</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">pll_inst</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="2261" delta="old" >The FF/Latch &lt;<arg fmt="%s" index="1">IR_code_0</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">ir_ct</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">13 FFs/Latches</arg>, which will be removed : <arg fmt="%s" index="4">&lt;IR_code_1&gt; &lt;IR_code_2&gt; &lt;IR_code_3&gt; &lt;IR_code_4&gt; &lt;IR_code_5&gt; &lt;IR_code_6&gt; &lt;IR_code_7&gt; &lt;IR_code_8&gt; &lt;IR_code_9&gt; &lt;IR_code_12&gt; &lt;IR_code_13&gt; &lt;IR_code_14&gt; &lt;IR_code_15&gt; </arg>
</msg>

<msg type="warning" file="Xst" num="1710" delta="old" >FF/Latch &lt;<arg fmt="%s" index="1">IR_code_0</arg>&gt; (without init value) has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">ir_ct</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_31</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_ct</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2404" delta="old" > FFs/Latches &lt;<arg fmt="%s" index="1">IR_code</arg>&lt;<arg fmt="%d" index="2">15</arg>:<arg fmt="%d" index="3">12</arg>&gt;&gt; (without init value) have a constant value of <arg fmt="%c" index="4">0</arg> in block &lt;<arg fmt="%s" index="5">ir_module</arg>&gt;.
</msg>

<msg type="info" file="Xst" num="3231" delta="old" >The small RAM &lt;<arg fmt="%s" index="1">Mram_ds_en[3]_num4[3]_mux_23_OUT</arg>&gt; will be implemented on LUTs in order to maximize performance and save block RAM resources. If you want to force its implementation on block, use option/constraint ram_style.
</msg>

<msg type="info" file="Xst" num="3231" delta="old" >The small RAM &lt;<arg fmt="%s" index="1">Mram_PWR_5_o_PWR_5_o_mux_16_OUT</arg>&gt; will be implemented on LUTs in order to maximize performance and save block RAM resources. If you want to force its implementation on block, use option/constraint ram_style.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_31</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="1710" delta="old" >FF/Latch &lt;<arg fmt="%s" index="1">IR_code_0</arg>&gt; (without init value) has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">ir_module</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1895" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">IR_code_1</arg>&gt; (without init value) has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">ir_module</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1895" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">IR_code_2</arg>&gt; (without init value) has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">ir_module</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1895" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">IR_code_3</arg>&gt; (without init value) has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">ir_module</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1895" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">IR_code_4</arg>&gt; (without init value) has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">ir_module</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1895" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">IR_code_5</arg>&gt; (without init value) has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">ir_module</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1895" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">IR_code_6</arg>&gt; (without init value) has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">ir_module</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1895" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">IR_code_7</arg>&gt; (without init value) has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">ir_module</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1895" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">IR_code_8</arg>&gt; (without init value) has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">ir_module</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1895" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">IR_code_9</arg>&gt; (without init value) has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">ir_module</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="info" file="Xst" num="2146" delta="old" >In block &lt;<arg fmt="%s" index="1">top</arg>&gt;, <arg fmt="%s" index="2">Counter</arg> &lt;<arg fmt="%s" index="3">cnt_5m12</arg>&gt; </msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_16</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_17</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_18</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_19</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_20</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_21</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_22</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_23</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_24</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_25</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_26</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_27</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_28</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_29</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">IR_Value_30</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">ir_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_17</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_18</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_19</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_20</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_21</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_22</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_23</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_24</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_25</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_26</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_27</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_28</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_29</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_30</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_31</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">dt_module</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_26</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">top</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_27</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">top</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_28</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">top</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_29</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">top</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_30</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">top</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">cnt_31</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">top</arg>&gt;.
</msg>

<msg type="info" file="Xst" num="1901" delta="new" >Instance <arg fmt="%s" index="1">pll_inst/pll_base_inst</arg> in unit <arg fmt="%s" index="2">pll_inst/pll_base_inst</arg> of type <arg fmt="%s" index="3">PLL_BASE</arg> has been replaced by <arg fmt="%s" index="4">PLL_ADV</arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_0</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_0&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_1</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_1&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_2</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_2&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_3</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_3&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_0</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_0&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_4</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_4&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_1</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_1&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_5</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_5&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_2</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_2&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_6</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_6&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_3</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_3&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_7</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_7&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_4</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_4&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_8</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_8&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_5</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_5&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_9</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_9&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_6</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_6&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_7</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_7&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_8</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_8&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_9</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_9&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_10</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_10&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_11</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_11&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_12</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_12&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_13</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_13&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_14</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_14&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_20</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_20&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_15</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_15&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_21</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_21&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_16</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_16&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_22</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_22&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_17</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_17&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_23</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_23&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_18</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_18&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_24</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_24&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_19</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_19&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_30</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_30&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_25</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_25&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_31</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_31&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_26</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_26&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_27</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_27&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_28</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_28&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/cnt_khz_29</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/cnt_29&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">beep_ct/clk_1k</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;key_ct/clk_khz&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_10</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_10&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_11</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_11&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_12</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_12&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_13</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_13&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_14</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_14&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_15</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_15&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">cnt_16</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">top</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;dt_ct/cnt_16&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2169" delta="old" >HDL ADVISOR - Some clock signals were not automatically buffered by XST with BUFG/BUFR resources. Please use the buffer_type constraint in order to insert these buffers to the clock signals to help prevent skew problems.
</msg>

</messages>

