##############################################################
#
# Xilinx Core Generator version 12.4
# Date: Fri Mar 21 13:11:00 2014
#
##############################################################
#
#  This file contains the customisation parameters for a
#  Xilinx CORE Generator IP GUI. It is strongly recommended
#  that you do not manually alter this file as it may cause
#  unexpected and unsupported behavior.
#
##############################################################
#
# BEGIN Project Options
SET addpads = false
SET asysymbol = true
SET busformat = BusFormatAngleBracketNotRipped
SET createndf = false
SET designentry = Verilog
SET device = xc6slx9
SET devicefamily = spartan6
SET flowvendor = Foundation_ISE
SET formalverification = false
SET foundationsym = false
SET implementationfiletype = Ngc
SET package = tqg144
SET removerpms = false
SET simulationfiles = Behavioral
SET speedgrade = -3
SET verilogsim = true
SET vhdlsim = true
# END Project Options
# BEGIN Select
SELECT Clocking_Wizard family Xilinx,_Inc. 1.8
# END Select
# BEGIN Parameters
CSET calc_done=DONE
CSET clk_out1_use_fine_ps_gui=false
CSET clk_out2_use_fine_ps_gui=false
CSET clk_out3_use_fine_ps_gui=false
CSET clk_out4_use_fine_ps_gui=false
CSET clk_out5_use_fine_ps_gui=false
CSET clk_out6_use_fine_ps_gui=false
CSET clk_out7_use_fine_ps_gui=false
CSET clkfb_in_signaling=SINGLE
CSET clkin1_jitter_ps=208.33
CSET clkin1_ui_jitter=0.010
CSET clkin2_jitter_ps=100.0
CSET clkin2_ui_jitter=0.010
CSET clkout1_drives=BUFG
CSET clkout1_requested_duty_cycle=50.000
CSET clkout1_requested_out_freq=40
CSET clkout1_requested_phase=0.000
CSET clkout2_drives=BUFG
CSET clkout2_requested_duty_cycle=50.000
CSET clkout2_requested_out_freq=16
CSET clkout2_requested_phase=0.000
CSET clkout2_used=true
CSET clkout3_drives=BUFG
CSET clkout3_requested_duty_cycle=50.000
CSET clkout3_requested_out_freq=5.12
CSET clkout3_requested_phase=0.000
CSET clkout3_used=true
CSET clkout4_drives=BUFG
CSET clkout4_requested_duty_cycle=50.000
CSET clkout4_requested_out_freq=5.12
CSET clkout4_requested_phase=0.000
CSET clkout4_used=false
CSET clkout5_drives=BUFG
CSET clkout5_requested_duty_cycle=50.000
CSET clkout5_requested_out_freq=100.000
CSET clkout5_requested_phase=0.000
CSET clkout5_used=false
CSET clkout6_drives=BUFG
CSET clkout6_requested_duty_cycle=50.000
CSET clkout6_requested_out_freq=100.000
CSET clkout6_requested_phase=0.000
CSET clkout6_used=false
CSET clkout7_drives=BUFG
CSET clkout7_requested_duty_cycle=50.000
CSET clkout7_requested_out_freq=100.000
CSET clkout7_requested_phase=0.000
CSET clkout7_used=false
CSET clock_mgr_type=AUTO
CSET component_name=clk_pll
CSET dcm_clk_feedback=1X
CSET dcm_clk_out1_port=CLKFX
CSET dcm_clk_out2_port=CLKDV
CSET dcm_clk_out3_port=CLK0
CSET dcm_clk_out4_port=CLK0
CSET dcm_clk_out5_port=CLK0
CSET dcm_clk_out6_port=CLK0
CSET dcm_clkdv_divide=3.0
CSET dcm_clkfx_divide=6
CSET dcm_clkfx_multiply=5
CSET dcm_clkgen_clk_out1_port=CLKFX
CSET dcm_clkgen_clk_out2_port=CLKFX
CSET dcm_clkgen_clk_out3_port=CLKFX
CSET dcm_clkgen_clkfx_divide=1
CSET dcm_clkgen_clkfx_md_max=0.000
CSET dcm_clkgen_clkfx_multiply=4
CSET dcm_clkgen_clkfxdv_divide=2
CSET dcm_clkgen_clkin_period=10.000
CSET dcm_clkgen_notes=None
CSET dcm_clkgen_spread_spectrum=NONE
CSET dcm_clkgen_startup_wait=false
CSET dcm_clkin_divide_by_2=false
CSET dcm_clkin_period=20.833
CSET dcm_clkout_phase_shift=NONE
CSET dcm_deskew_adjust=SYSTEM_SYNCHRONOUS
CSET dcm_notes=None
CSET dcm_phase_shift=0
CSET dcm_startup_wait=false
CSET feedback_source=FDBK_AUTO
CSET in_freq_units=Units_MHz
CSET in_jitter_units=Units_UI
CSET jitter_options=UI
CSET jitter_sel=No_Jitter
CSET mmcm_bandwidth=OPTIMIZED
CSET mmcm_clkfbout_mult_f=4.000
CSET mmcm_clkfbout_phase=0.000
CSET mmcm_clkfbout_use_fine_ps=false
CSET mmcm_clkin1_period=10.000
CSET mmcm_clkin2_period=10.000
CSET mmcm_clkout0_divide_f=4.000
CSET mmcm_clkout0_duty_cycle=0.500
CSET mmcm_clkout0_phase=0.000
CSET mmcm_clkout0_use_fine_ps=false
CSET mmcm_clkout1_divide=1
CSET mmcm_clkout1_duty_cycle=0.500
CSET mmcm_clkout1_phase=0.000
CSET mmcm_clkout1_use_fine_ps=false
CSET mmcm_clkout2_divide=1
CSET mmcm_clkout2_duty_cycle=0.500
CSET mmcm_clkout2_phase=0.000
CSET mmcm_clkout2_use_fine_ps=false
CSET mmcm_clkout3_divide=1
CSET mmcm_clkout3_duty_cycle=0.500
CSET mmcm_clkout3_phase=0.000
CSET mmcm_clkout3_use_fine_ps=false
CSET mmcm_clkout4_cascade=false
CSET mmcm_clkout4_divide=1
CSET mmcm_clkout4_duty_cycle=0.500
CSET mmcm_clkout4_phase=0.000
CSET mmcm_clkout4_use_fine_ps=false
CSET mmcm_clkout5_divide=1
CSET mmcm_clkout5_duty_cycle=0.500
CSET mmcm_clkout5_phase=0.000
CSET mmcm_clkout5_use_fine_ps=false
CSET mmcm_clkout6_divide=1
CSET mmcm_clkout6_duty_cycle=0.500
CSET mmcm_clkout6_phase=0.000
CSET mmcm_clkout6_use_fine_ps=false
CSET mmcm_clock_hold=false
CSET mmcm_compensation=ZHOLD
CSET mmcm_divclk_divide=1
CSET mmcm_notes=None
CSET mmcm_ref_jitter1=0.010
CSET mmcm_ref_jitter2=0.010
CSET mmcm_startup_wait=false
CSET num_out_clks=3
CSET override_dcm=false
CSET override_dcm_clkgen=false
CSET override_mmcm=false
CSET override_pll=false
CSET platform=nt64
CSET pll_bandwidth=OPTIMIZED
CSET pll_clk_feedback=CLKFBOUT
CSET pll_clkfbout_mult=10
CSET pll_clkfbout_phase=0.000
CSET pll_clkin_period=20.833
CSET pll_clkout0_divide=12
CSET pll_clkout0_duty_cycle=0.500
CSET pll_clkout0_phase=0.000
CSET pll_clkout1_divide=30
CSET pll_clkout1_duty_cycle=0.500
CSET pll_clkout1_phase=0.000
CSET pll_clkout2_divide=94
CSET pll_clkout2_duty_cycle=0.500
CSET pll_clkout2_phase=0.000
CSET pll_clkout3_divide=94
CSET pll_clkout3_duty_cycle=0.500
CSET pll_clkout3_phase=0.000
CSET pll_clkout4_divide=1
CSET pll_clkout4_duty_cycle=0.500
CSET pll_clkout4_phase=0.000
CSET pll_clkout5_divide=1
CSET pll_clkout5_duty_cycle=0.500
CSET pll_clkout5_phase=0.000
CSET pll_compensation=SYSTEM_SYNCHRONOUS
CSET pll_divclk_divide=1
CSET pll_notes=None
CSET pll_ref_jitter=0.010
CSET prim_in_freq=48
CSET prim_in_jitter=0.010
CSET prim_source=Global_buffer
CSET primtype_sel=PLL_BASE
CSET relative_inclk=REL_PRIMARY
CSET secondary_in_freq=100.000
CSET secondary_in_jitter=0.010
CSET secondary_source=Single_ended_clock_capable_pin
CSET summary_strings=empty
CSET use_clk_valid=false
CSET use_dyn_phase_shift=false
CSET use_dyn_reconfig=false
CSET use_freeze=false
CSET use_freq_synth=true
CSET use_inclk_stopped=false
CSET use_inclk_switchover=false
CSET use_locked=true
CSET use_max_i_jitter=false
CSET use_min_o_jitter=false
CSET use_min_power=false
CSET use_phase_alignment=true
CSET use_power_down=false
CSET use_reset=true
CSET use_spread_spectrum=false
CSET use_status=false
# END Parameters
GENERATE
# CRC: 873718f5
