<?xml version="1.0" encoding="UTF-8"?>
<!-- IMPORTANT: This is an internal file that has been generated
     by the Xilinx ISE software.  Any direct editing or
     changes made to this file may result in unpredictable
     behavior or data corruption.  It is strongly advised that
     users do not edit the contents of this file. -->
<messages>
<msg type="warning" file="Xst" num="916" delta="new" >&quot;<arg fmt="%s" index="1">sdrm.v</arg>&quot; line <arg fmt="%d" index="2">162</arg>: Delay is ignored for synthesis.
</msg>

<msg type="warning" file="Xst" num="916" delta="new" >&quot;<arg fmt="%s" index="1">sdrm.v</arg>&quot; line <arg fmt="%d" index="2">165</arg>: Delay is ignored for synthesis.
</msg>

<msg type="warning" file="Xst" num="916" delta="new" >&quot;<arg fmt="%s" index="1">sdrm.v</arg>&quot; line <arg fmt="%d" index="2">166</arg>: Delay is ignored for synthesis.
</msg>

<msg type="warning" file="Xst" num="916" delta="new" >&quot;<arg fmt="%s" index="1">sdrm.v</arg>&quot; line <arg fmt="%d" index="2">167</arg>: Delay is ignored for synthesis.
</msg>

<msg type="warning" file="Xst" num="916" delta="new" >&quot;<arg fmt="%s" index="1">sdrm.v</arg>&quot; line <arg fmt="%d" index="2">168</arg>: Delay is ignored for synthesis.
</msg>

<msg type="warning" file="Xst" num="915" delta="new" >Message (<arg fmt="%d" index="1">916</arg>) is reported only 5 times for each module.
</msg>

<msg type="warning" file="Xst" num="916" delta="new" >&quot;<arg fmt="%s" index="1">sdrm_t.v</arg>&quot; line <arg fmt="%d" index="2">136</arg>: Delay is ignored for synthesis.
</msg>

<msg type="warning" file="Xst" num="916" delta="new" >&quot;<arg fmt="%s" index="1">sdrm_t.v</arg>&quot; line <arg fmt="%d" index="2">137</arg>: Delay is ignored for synthesis.
</msg>

<msg type="warning" file="Xst" num="916" delta="new" >&quot;<arg fmt="%s" index="1">sdrm_t.v</arg>&quot; line <arg fmt="%d" index="2">138</arg>: Delay is ignored for synthesis.
</msg>

<msg type="warning" file="Xst" num="916" delta="new" >&quot;<arg fmt="%s" index="1">sdrm_t.v</arg>&quot; line <arg fmt="%d" index="2">139</arg>: Delay is ignored for synthesis.
</msg>

<msg type="warning" file="Xst" num="916" delta="new" >&quot;<arg fmt="%s" index="1">sdrm_t.v</arg>&quot; line <arg fmt="%d" index="2">142</arg>: Delay is ignored for synthesis.
</msg>

<msg type="warning" file="Xst" num="915" delta="new" >Message (<arg fmt="%d" index="1">916</arg>) is reported only 5 times for each module.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">we_rn_reg</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">data_addr_n_i</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="646" delta="new" >Signal &lt;<arg fmt="%s" index="1">cntrl&lt;31:28&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="new" >Signal &lt;<arg fmt="%s" index="1">cntrl&lt;7&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="new" >Signal &lt;<arg fmt="%s" index="1">unused3</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="new" >Signal &lt;<arg fmt="%s" index="1">unused2</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="new" >Signal &lt;<arg fmt="%s" index="1">unused1</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="new" >Signal &lt;<arg fmt="%s" index="1">ready_o</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="new" >Signal &lt;<arg fmt="%s" index="1">rcd_end</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="new" >Signal &lt;<arg fmt="%s" index="1">kid</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="new" >Signal &lt;<arg fmt="%s" index="1">Locked_j</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="new" >Signal &lt;<arg fmt="%s" index="1">Add_reg&lt;31:22&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="new" >Signal &lt;<arg fmt="%s" index="1">Add_reg&lt;1:0&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">sd_doe_n_0</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">sdrm_t</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">3 FFs/Latches</arg>, which will be removed : <arg fmt="%s" index="4">&lt;sd_doe_n_1&gt; &lt;sd_doe_n_2&gt; &lt;sd_doe_n_3&gt; </arg>
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_0</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_1</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_22</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_23</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_24</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_25</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_26</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_27</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_28</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_29</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_30</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">Add_reg_31</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="info" file="Xst" num="3034" delta="new" >In order to maximize performance and save block RAM resources, the small ROM &lt;<arg fmt="%s" index="1">Mrom_Act_st_mux0000</arg>&gt; will be implemented on LUT. If you want to force its implementation on block, use option/constraint rom_style.
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">sd_doe_n_0</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">sdrm_t</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">3 FFs/Latches</arg>, which will be removed : <arg fmt="%s" index="4">&lt;sd_doe_n_1&gt; &lt;sd_doe_n_2&gt; &lt;sd_doe_n_3&gt; </arg>
</msg>

<msg type="info" file="Xst" num="1901" delta="new" >Instance <arg fmt="%s" index="1">dll0</arg> in unit <arg fmt="%s" index="2">sdrm</arg> of type <arg fmt="%s" index="3">DCM_BASE</arg> has been replaced by <arg fmt="%s" index="4">DCM_ADV</arg>
</msg>

<msg type="info" file="Xst" num="1901" delta="new" >Instance <arg fmt="%s" index="1">dll1</arg> in unit <arg fmt="%s" index="2">sdrm</arg> of type <arg fmt="%s" index="3">DCM_BASE</arg> has been replaced by <arg fmt="%s" index="4">DCM_ADV</arg>
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">cntrl_31</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">cntrl_30</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">cntrl_29</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">cntrl_28</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">cntrl_7</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sys_int</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">we_rn_reg</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_31</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_30</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_29</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_28</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_27</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_26</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_25</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_24</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_23</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_22</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_1</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sys_int/Add_reg_0</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sdrm_t/ref_cntr/p_auto_ref</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">sdrm_t/ready_o</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">sdrm</arg>&gt;.
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">sd_doe_n_0</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">sdrm</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">3 FFs/Latches</arg>, which will be removed : <arg fmt="%s" index="4">&lt;sd_doe_n_1&gt; &lt;sd_doe_n_2&gt; &lt;sd_doe_n_3&gt; </arg>
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">sd_data_t_24</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">sdrm</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">3 FFs/Latches</arg>, which will be removed : <arg fmt="%s" index="4">&lt;sd_data_t_16&gt; &lt;sd_data_t_10&gt; &lt;sd_data_t_0&gt; </arg>
</msg>

<msg type="info" file="Xst" num="1843" delta="new" >HDL ADVISOR - FlipFlop <arg fmt="%s" index="1">data_addr_n_reg</arg> connected to a primary input has been replicated
</msg>

</messages>

