Device Usage Statistics Report

### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:14.7 (WebPack) - P.20131013 | Target Family: | Spartan6
OS Platform: | NT64 | Target Device: | xc6slx9
Project ID (random number) | 9af4f16000124bd594554d52cdb242aa. D9869C593B82457BB0679FEF5A9DB123. 3 | Target Package: | tqg144
Registration ID | __0_0_0 | Target Speed: | -3
Date Generated | 2014-06-20T21:46:06 | Tool Flow | ISE

User Environment
OS Name | Microsoft Windows 7 , 64-bit | OS Release | Service Pack 1 (build 7601)
CPU Name | AMD A8-5600K APU with Radeon(tm) HD Graphics | CPU Speed | 3600 MHz
OS Name | Microsoft Windows 7 , 64-bit | OS Release | Service Pack 1 (build 7601)
CPU Name | AMD A8-5600K APU with Radeon(tm) HD Graphics | CPU Speed | 3600 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage

MiscellaneousStatistics

- AGG_BONDED_IO=4
- AGG_IO=4
- AGG_LOCED_IO=4
- NUM_BONDED_IOB=4
- NUM_LOCED_IOB=4

NetStatistics

- NumNets_Active=4
- NumNets_Gnd=1
- NumNets_Vcc=1
- NumNodesOfType_Gnd_DOUBLE=1
- NumNodesOfType_Gnd_GENERIC=2
- NumNodesOfType_Gnd_IOBIN2OUT=2
- NumNodesOfType_Gnd_IOBOUTPUT=2
- NumNodesOfType_Gnd_OUTBOUND=2
- NumNodesOfType_Gnd_OUTPUT=2
- NumNodesOfType_Gnd_PADINPUT=2
- NumNodesOfType_Gnd_PINFEED=2
- NumNodesOfType_Gnd_SINGLE=1
- NumNodesOfType_Vcc_GENERIC=2
- NumNodesOfType_Vcc_HVCCOUT=1
- NumNodesOfType_Vcc_IOBIN2OUT=2
- NumNodesOfType_Vcc_IOBOUTPUT=2
- NumNodesOfType_Vcc_PADINPUT=2
- NumNodesOfType_Vcc_PINFEED=2

SiteStatistics

- IOB-IOBM=2
- IOB-IOBS=2

SiteSummary

- IOB=4
- IOB_OUTBUF=4
- PAD=4

Configuration Data

IOB_OUTBUF

- DRIVEATTRBOX=[12:4]
- SLEW=[SLOW:4]
- SUSPEND=[3STATE:4]

Pin Data

IOB

- O=4
- PAD=4

IOB_OUTBUF

- IN=4
- OUT=4

PAD

- PAD=4

Tool Usage

Command Line History

- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx9-tqg144-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 3 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx9-tqg144-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx9-tqg144-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 3 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd

Software Quality
Run Statistics
Program Name | Runs Started | Runs Finished | Errors | Fatal Errors | Internal Errors | Exceptions | Core Dumps
_impact | 19 | 8 | 0 | 0 | 0 | 0 | 0
bitgen | 7 | 7 | 0 | 0 | 0 | 0 | 0
cse_server | 4 | 4 | 0 | 0 | 0 | 0 | 0
map | 12 | 7 | 0 | 0 | 0 | 0 | 0
ngcbuild | 11 | 11 | 0 | 0 | 0 | 0 | 0
ngdbuild | 15 | 15 | 0 | 0 | 0 | 0 | 0
par | 7 | 7 | 0 | 0 | 0 | 0 | 0
trce | 6 | 6 | 0 | 0 | 0 | 0 | 0
xst | 14 | 12 | 0 | 0 | 0 | 0 | 0

Help Statistics
Help files
/doc/usenglish/isehelp/pim_c_arranging_windows.htm ( 1 ) | /doc/usenglish/isehelp/pim_c_device_configuration.htm ( 1 )
/doc/usenglish/isehelp/pim_c_overview.htm ( 1 ) | /doc/usenglish/isehelp/pim_c_webtalk_in_impact.htm ( 1 )
/doc/usenglish/isehelp/pim_db_impact_wizard.htm ( 1 ) | /doc/usenglish/isehelp/pim_p_accessing_impact_from_command_line_prompt.htm ( 1 )
/doc/usenglish/isehelp/pim_p_creating_a_new_projectfile.htm ( 1 ) | /doc/usenglish/isehelp/pim_p_loading_project_files.htm ( 1 )
/doc/usenglish/isehelp/pim_p_opening_impact_project.htm ( 1 ) | /doc/usenglish/isehelp/pim_r_configurationtabs.htm ( 1 )
/doc/usenglish/isehelp/pim_r_console_comds.htm ( 1 ) | /doc/usenglish/isehelp/pim_r_impactfiles.htm ( 1 )
/doc/usenglish/isehelp/pim_r_short.htm ( 1 ) | /doc/usenglish/isehelp/pim_r_supportedcables.htm ( 1 )
/doc/usenglish/isehelp/pim_r_toolbar.htm ( 1 )

Project Statistics
PROP_Enable_Message_Filtering= false | PROP_FitterReportFormat= HTML
PROP_LastAppliedGoal= Balanced | PROP_LastAppliedStrategy= Xilinx Default (unlocked)
PROP_ManualCompileOrderImp= false | PROP_PropSpecInProjFile= Store all values
PROP_Simulator= Modelsim-SE Verilog | PROP_SynthTopFile= changed
PROP_Top_Level_Module_Type= HDL | PROP_UseSmartGuide= false
PROP_UserConstraintEditorPreference= Text Editor | PROP_intProjectCreationTimestamp= 2014-06-20T19:47:00
PROP_intWbtProjectID= D9869C593B82457BB0679FEF5A9DB123 | PROP_intWbtProjectIteration= 3
PROP_intWorkingDirLocWRTProjDir= Same | PROP_intWorkingDirUsed= No
PROP_AutoTop= true | PROP_DevFamily= Spartan6
PROP_DevDevice= xc6slx9 | PROP_DevFamilyPMName= spartan6
PROP_DevPackage= tqg144 | PROP_Synthesis_Tool= XST (VHDL/Verilog)
PROP_DevSpeed=-3 | PROP_PreferredLanguage= Verilog
FILE_UCF= 1 | FILE_VERILOG= 1

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_GND= 1 | NGDBUILD_NUM_OBUF= 4 | NGDBUILD_NUM_VCC= 1
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_GND= 1 | NGDBUILD_NUM_OBUF= 4 | NGDBUILD_NUM_VCC= 1

XST Command Line Options
XST_OPTION_SUMMARY
-ifn=<fname>.prj | -ofn=<design_top> | -ofmt= NGC | -p= xc6slx9-3-tqg144
-top=<design_top> | -opt_mode= Speed | -opt_level= 1 | -power= NO
-iuc= NO | -keep_hierarchy= No | -netlist_hierarchy= As_Optimized | -rtlview= Yes
-glob_opt= AllClockNets | -read_cores= YES | -write_timing_constraints= NO | -cross_clock_analysis= NO
-bus_delimiter=<> | -slice_utilization_ratio= 100 | -bram_utilization_ratio= 100 | -dsp_utilization_ratio= 100
-reduce_control_sets= Auto | -fsm_extract= YES | -fsm_encoding= Auto | -safe_implementation= No
-fsm_style= LUT | -ram_extract= Yes | -ram_style= Auto | -rom_extract= Yes
-shreg_extract= YES | -rom_style= Auto | -auto_bram_packing= NO | -resource_sharing= YES
-async_to_sync= NO | -use_dsp48= Auto | -iobuf= YES | -max_fanout= 100000
-bufg= 16 | -register_duplication= YES | -register_balancing= No | -optimize_primitives= NO
-use_clock_enable= Auto | -use_sync_set= Auto | -use_sync_reset= Auto | -iob= Auto
-equivalent_register_removal= YES | -slice_utilization_ratio_maxmargin= 5