Device Usage Statistics Report

### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:14.7 (WebPack) - P.20131013 | Target Family: | Spartan6
OS Platform: | NT64 | Target Device: | xc6slx9
Project ID (random number) | 9af4f16000124bd594554d52cdb242aa. D9869C593B82457BB0679FEF5A9DB123. 6 | Target Package: | tqg144
Registration ID | __0_0_0 | Target Speed: | -3
Date Generated | 2014-06-20T22:15:32 | Tool Flow | ISE

User Environment
OS Name | Microsoft Windows 7 , 64-bit | OS Release | Service Pack 1 (build 7601)
CPU Name | AMD A8-5600K APU with Radeon(tm) HD Graphics | CPU Speed | 3600 MHz
OS Name | Microsoft Windows 7 , 64-bit | OS Release | Service Pack 1 (build 7601)
CPU Name | AMD A8-5600K APU with Radeon(tm) HD Graphics | CPU Speed | 3600 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage

Counters=1

- 32-bit up counter=1

Registers=1

- Flip-Flops=1

MiscellaneousStatistics

- AGG_BONDED_IO=5
- AGG_IO=5
- AGG_LOCED_IO=5
- AGG_SLICE=17
- NUM_BONDED_IOB=5
- NUM_BSFULL=27
- NUM_BSLUTONLY=33
- NUM_BSUSED=60
- NUM_BUFG=1
- NUM_LOCED_IOB=5
- NUM_LOGIC_O5ANDO6=1
- NUM_LOGIC_O5ONLY=23
- NUM_LOGIC_O6ONLY=35
- NUM_LUT_RT_DRIVES_CARRY4=1
- NUM_LUT_RT_EXO6=1
- NUM_LUT_RT_O6=23
- NUM_SLICEL=7
- NUM_SLICEX=10
- NUM_SLICE_CARRY4=7
- NUM_SLICE_CONTROLSET=1
- NUM_SLICE_CYINIT=85
- NUM_SLICE_FF=27
- NUM_SLICE_UNUSEDCTRL=9
- NUM_UNUSABLE_FF_BELS=5

NetStatistics

- NumNets_Active=75
- NumNets_Vcc=1
- NumNodesOfType_Active_BOUNCEACROSS=2
- NumNodesOfType_Active_BOUNCEIN=14
- NumNodesOfType_Active_BUFGOUT=1
- NumNodesOfType_Active_BUFHINP2OUT=1
- NumNodesOfType_Active_CLKPIN=8
- NumNodesOfType_Active_CLKPINFEED=1
- NumNodesOfType_Active_DOUBLE=58
- NumNodesOfType_Active_GENERIC=5
- NumNodesOfType_Active_GLOBAL=9
- NumNodesOfType_Active_INPUT=7
- NumNodesOfType_Active_IOBIN2OUT=4
- NumNodesOfType_Active_IOBOUTPUT=4
- NumNodesOfType_Active_LUTINPUT=235
- NumNodesOfType_Active_OUTBOUND=64
- NumNodesOfType_Active_OUTPUT=71
- NumNodesOfType_Active_PADINPUT=4
- NumNodesOfType_Active_PADOUTPUT=1
- NumNodesOfType_Active_PINBOUNCE=30
- NumNodesOfType_Active_PINFEED=248
- NumNodesOfType_Active_QUAD=7
- NumNodesOfType_Active_REGINPUT=1
- NumNodesOfType_Active_SINGLE=126

SiteStatistics

- BUFG-BUFGMUX=1
- IOB-IOBM=3
- IOB-IOBS=2
- SLICEL-SLICEM=7
- SLICEX-SLICEL=4

SiteSummary

- BUFG=1
- BUFG_BUFG=1
- CARRY4=7
- HARD0=1
- IOB=5
- IOB_IMUX=1
- IOB_INBUF=1
- IOB_OUTBUF=4
- LUT5=24
- LUT6=60
- PAD=5
- REG_SR=27
- SLICEL=7
- SLICEX=10

Configuration Data

IOB_OUTBUF

- DRIVEATTRBOX=[12:4]
- SLEW=[SLOW:4]
- SUSPEND=[3STATE:4]

REG_SR

- CK=[CK:27] [CK_INV:0]
- LATCH_OR_FF=[FF:27]
- SRINIT=[SRINIT0:27]
- SYNC_ATTR=[ASYNC:27]

SLICEX

- CLK=[CLK:8] [CLK_INV:0]

Pin Data

BUFG

- I0=1
- O=1

BUFG_BUFG

- I0=1
- O=1

CARRY4

- CIN=6
- CO3=6
- CYINIT=1
- DI0=6
- DI1=6
- DI2=6
- DI3=6
- O0=7
- O1=6
- O2=6
- O3=6
- S0=7
- S1=6
- S2=6
- S3=6

HARD0

- 0=1

IOB

- I=1
- O=4
- PAD=5

IOB_IMUX

- I=1
- OUT=1

IOB_INBUF

- OUT=1
- PAD=1

IOB_OUTBUF

- IN=4
- OUT=4

LUT5

- O5=24

LUT6

- A1=35
- A2=35
- A3=35
- A4=35
- A5=59
- A6=60
- O6=60

PAD

- PAD=5

REG_SR

- CK=27
- D=27
- Q=27

SLICEL

- A5=6
- A6=7
- AMUX=7
- B5=6
- B6=6
- BMUX=6
- C5=6
- C6=6
- CIN=6
- CMUX=6
- COUT=6
- D5=6
- D6=6
- DMUX=6

SLICEX

- A=2
- A1=9
- A2=9
- A3=9
- A4=9
- A5=9
- A6=9
- AQ=7
- B=3
- B1=9
- B2=9
- B3=9
- B4=9
- B5=9
- B6=9
- BQ=7
- BX=1
- C=2
- C1=8
- C2=8
- C3=8
- C4=8
- C5=8
- C6=8
- CLK=8
- CQ=6
- D=3
- D1=9
- D2=9
- D3=9
- D4=9
- D5=9
- D6=9
- DQ=7

Tool Usage

Command Line History

- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx9-tqg144-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 3 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx9-tqg144-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx9-tqg144-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 3 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx9-tqg144-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 3 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx9-tqg144-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 3 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx9-tqg144-3 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx9-tqg144-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 3 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd

Software Quality
Run Statistics
Program Name | Runs Started | Runs Finished | Errors | Fatal Errors | Internal Errors | Exceptions | Core Dumps
_impact | 20 | 10 | 0 | 0 | 0 | 0 | 0
bitgen | 10 | 10 | 0 | 0 | 0 | 0 | 0
cse_server | 4 | 4 | 0 | 0 | 0 | 0 | 0
map | 15 | 10 | 0 | 0 | 0 | 0 | 0
ngcbuild | 11 | 11 | 0 | 0 | 0 | 0 | 0
ngdbuild | 19 | 19 | 0 | 0 | 0 | 0 | 0
par | 10 | 10 | 0 | 0 | 0 | 0 | 0
trce | 9 | 9 | 0 | 0 | 0 | 0 | 0
xst | 18 | 16 | 0 | 0 | 0 | 0 | 0

Help Statistics
Help files
/doc/usenglish/isehelp/pim_c_arranging_windows.htm ( 1 ) | /doc/usenglish/isehelp/pim_c_device_configuration.htm ( 1 )
/doc/usenglish/isehelp/pim_c_overview.htm ( 1 ) | /doc/usenglish/isehelp/pim_c_webtalk_in_impact.htm ( 1 )
/doc/usenglish/isehelp/pim_db_impact_wizard.htm ( 1 ) | /doc/usenglish/isehelp/pim_p_accessing_impact_from_command_line_prompt.htm ( 1 )
/doc/usenglish/isehelp/pim_p_creating_a_new_projectfile.htm ( 1 ) | /doc/usenglish/isehelp/pim_p_loading_project_files.htm ( 1 )
/doc/usenglish/isehelp/pim_p_opening_impact_project.htm ( 1 ) | /doc/usenglish/isehelp/pim_r_configurationtabs.htm ( 1 )
/doc/usenglish/isehelp/pim_r_console_comds.htm ( 1 ) | /doc/usenglish/isehelp/pim_r_impactfiles.htm ( 1 )
/doc/usenglish/isehelp/pim_r_short.htm ( 1 ) | /doc/usenglish/isehelp/pim_r_supportedcables.htm ( 1 )
/doc/usenglish/isehelp/pim_r_toolbar.htm ( 1 )

Project Statistics
PROP_Enable_Message_Filtering= false | PROP_FitterReportFormat= HTML
PROP_LastAppliedGoal= Balanced | PROP_LastAppliedStrategy= Xilinx Default (unlocked)
PROP_ManualCompileOrderImp= false | PROP_PropSpecInProjFile= Store all values
PROP_Simulator= Modelsim-SE Verilog | PROP_SynthTopFile= changed
PROP_Top_Level_Module_Type= HDL | PROP_UseSmartGuide= false
PROP_UserConstraintEditorPreference= Text Editor | PROP_intProjectCreationTimestamp= 2014-06-20T19:47:00
PROP_intWbtProjectID= D9869C593B82457BB0679FEF5A9DB123 | PROP_intWbtProjectIteration= 6
PROP_intWorkingDirLocWRTProjDir= Same | PROP_intWorkingDirUsed= No
PROP_xilxBitgStart_IntDone= true | PROP_AutoTop= true
PROP_DevFamily= Spartan6 | PROP_DevDevice= xc6slx9
PROP_DevFamilyPMName= spartan6 | PROP_DevPackage= tqg144
PROP_Synthesis_Tool= XST (VHDL/Verilog) | PROP_DevSpeed=-3
PROP_PreferredLanguage= Verilog | FILE_UCF= 1
FILE_VERILOG= 1

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_BUFGP= 1 | NGDBUILD_NUM_FD= 27 | NGDBUILD_NUM_GND= 1 | NGDBUILD_NUM_INV= 1
NGDBUILD_NUM_LUT1= 24 | NGDBUILD_NUM_LUT6= 35 | NGDBUILD_NUM_MUXCY= 24 | NGDBUILD_NUM_OBUF= 4
NGDBUILD_NUM_VCC= 1 | NGDBUILD_NUM_XORCY= 25
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG= 1 | NGDBUILD_NUM_FD= 27 | NGDBUILD_NUM_GND= 1 | NGDBUILD_NUM_IBUFG= 1
NGDBUILD_NUM_INV= 1 | NGDBUILD_NUM_LUT1= 24 | NGDBUILD_NUM_LUT6= 35 | NGDBUILD_NUM_MUXCY= 24
NGDBUILD_NUM_OBUF= 4 | NGDBUILD_NUM_VCC= 1 | NGDBUILD_NUM_XORCY= 25

XST Command Line Options
XST_OPTION_SUMMARY
-ifn=<fname>.prj | -ofn=<design_top> | -ofmt= NGC | -p= xc6slx9-3-tqg144
-top=<design_top> | -opt_mode= Speed | -opt_level= 1 | -power= NO
-iuc= NO | -keep_hierarchy= No | -netlist_hierarchy= As_Optimized | -rtlview= Yes
-glob_opt= AllClockNets | -read_cores= YES | -write_timing_constraints= NO | -cross_clock_analysis= NO
-bus_delimiter=<> | -slice_utilization_ratio= 100 | -bram_utilization_ratio= 100 | -dsp_utilization_ratio= 100
-reduce_control_sets= Auto | -fsm_extract= YES | -fsm_encoding= Auto | -safe_implementation= No
-fsm_style= LUT | -ram_extract= Yes | -ram_style= Auto | -rom_extract= Yes
-shreg_extract= YES | -rom_style= Auto | -auto_bram_packing= NO | -resource_sharing= YES
-async_to_sync= NO | -use_dsp48= Auto | -iobuf= YES | -max_fanout= 100000
-bufg= 16 | -register_duplication= YES | -register_balancing= No | -optimize_primitives= NO
-use_clock_enable= Auto | -use_sync_set= Auto | -use_sync_reset= Auto | -iob= Auto
-equivalent_register_removal= YES | -slice_utilization_ratio_maxmargin= 5