Par Statistics
Total Non-vccgnd Signals= 87
Total Non-vccgnd Design Pins= 180
Total Non-vccgnd Conns= 180
Total Non-vccgnd Timing Constrained Conns= 176
Phase 1 CPU= 5.4 sec
Phase 2 CPU= 5.4 sec
Phase 3 CPU= 5.6 sec
Phase 4 CPU= 6.1 sec
Phase 5 CPU= 6.3 sec
Phase 6 CPU= 6.3 sec
Phase 7 CPU= 6.3 sec
Phase 8 CPU= 6.3 sec
Phase 9 CPU= 6.3 sec
Phase 10 CPU= 6.3 sec
AvgWirelenPerPin Fanout 1= 1.0
AvgWirelenPerPin Fanout 2= 0.5
AvgWirelenPerPin Fanout 3= 2.7
AvgWirelenPerPin Fanout 4= 0.0
AvgWirelenPerPin Fanout 10= 4.8
AvgWirelenPerPin Fanout 50= 0.7
AvgWirelenPerPin Fanout 100= 0.0
AvgWirelenPerPin Fanout 500= 0.0
AvgWirelenPerPin Fanout 5000= 0.0
AvgWirelenPerPin Fanout 20000= 0.0
AvgWirelenPerPin Fanout 50000= 0.0
AvgWirelenPerPin Fanout 100000= 0.0
IRR Gamma= 1.0141