Par Statistics
Total Non-vccgnd Signals= 436
Total Non-vccgnd Design Pins= 955
Total Non-vccgnd Conns= 955
Total Non-vccgnd Timing Constrained Conns= 760
Phase 1 CPU= 5.0 sec
Phase 2 CPU= 5.2 sec
Phase 3 CPU= 6.0 sec
Phase 4 CPU= 6.5 sec
Phase 5 CPU= 7.1 sec
Phase 6 CPU= 7.1 sec
Phase 7 CPU= 7.1 sec
Phase 8 CPU= 7.1 sec
Phase 9 CPU= 7.1 sec
Phase 10 CPU= 7.2 sec
AvgWirelenPerPin Fanout 1= 1.0
AvgWirelenPerPin Fanout 2= 0.5
AvgWirelenPerPin Fanout 3= 2.0
AvgWirelenPerPin Fanout 4= 1.3
AvgWirelenPerPin Fanout 10= 1.9
AvgWirelenPerPin Fanout 50= 2.5
AvgWirelenPerPin Fanout 100= 0.0
AvgWirelenPerPin Fanout 500= 0.0
AvgWirelenPerPin Fanout 5000= 0.0
AvgWirelenPerPin Fanout 20000= 0.0
AvgWirelenPerPin Fanout 50000= 0.0
AvgWirelenPerPin Fanout 100000= 0.0
IRR Gamma= 1.0882