<?xml version="1.0" encoding="UTF-8"?>
<!-- IMPORTANT: This is an internal file that has been generated
     by the Xilinx ISE software.  Any direct editing or
     changes made to this file may result in unpredictable
     behavior or data corruption.  It is strongly advised that
     users do not edit the contents of this file. -->
<messages>
<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\chipscope_ila.vhd" Line 292: Assignment to <arg fmt="%s" index="1">logic_1</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_reset_ctrl.vhd" Line 88: Assignment to <arg fmt="%s" index="1">logic_1</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_match.vhd" Line 93: Assignment to <arg fmt="%s" index="1">logic_0</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_match_varx.vhd" Line 80: Assignment to <arg fmt="%s" index="1">logic_1</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_match_varx.vhd" Line 82: Assignment to <arg fmt="%s" index="1">logic_0</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_match_varx_srl32.vhd" Line 117: Assignment to <arg fmt="%s" index="1">logic_0</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_match_var_srl32.vhd" Line 83: Assignment to <arg fmt="%s" index="1">logic_0</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_match.vhd" Line 306: Net &lt;<arg fmt="%s" index="1">I_MUT_VARX.MODE_Q</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_trigcond.vhd" Line 120: Assignment to <arg fmt="%s" index="1">logic_1</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_trigcond.vhd" Line 110: Net &lt;<arg fmt="%s" index="1">iCFG_EN_VEC[15]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_match_gand.vhd" Line 83: Assignment to <arg fmt="%s" index="1">logic_1</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_match_gand.vhd" Line 84: Assignment to <arg fmt="%s" index="1">logic_0</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="871" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_lib_v1_03_a\cs_gand_srl_s6.vhd" Line 64: Using initial value <arg fmt="%s" index="1">&apos;1&apos;</arg> for <arg fmt="%s" index="2">logic_1</arg> since it is never assigned
</msg>

<msg type="warning" file="HDLCompiler" num="871" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_lib_v1_03_a\cs_gand_srl_s6_rpm_set.vhd" Line 156: Using initial value <arg fmt="%s" index="1">&quot;1111111&quot;</arg> for <arg fmt="%s" index="2">srl_remainder</arg> since it is never assigned
</msg>

<msg type="warning" file="HDLCompiler" num="871" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_lib_v1_03_a\cs_gand_srl_s6_slice.vhd" Line 76: Using initial value <arg fmt="%s" index="1">&apos;1&apos;</arg> for <arg fmt="%s" index="2">logic_1</arg> since it is never assigned
</msg>

<msg type="warning" file="HDLCompiler" num="871" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_lib_v1_03_a\cs_gand_srl_s6_slice.vhd" Line 77: Using initial value <arg fmt="%s" index="1">&apos;0&apos;</arg> for <arg fmt="%s" index="2">logic_0</arg> since it is never assigned
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_cap_storage.vhd" Line 183: Assignment to <arg fmt="%s" index="1">logic_1</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="1127" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_cap_storage.vhd" Line 184: Assignment to <arg fmt="%s" index="1">logic_0</arg> ignored, since the identifier is never used
</msg>

<msg type="warning" file="HDLCompiler" num="89" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_lib_v1_03_a\cs_bram_simple_s6_ramb9.vhd" Line 130: &lt;<arg fmt="%s" index="1">ramb8bwer</arg>&gt; remains a black-box since it has no binding entity.
</msg>

<msg type="warning" file="HDLCompiler" num="746" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_trace_buffer.vhd" Line 201: Range is empty (null range)
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_core.vhd" Line 383: Net &lt;<arg fmt="%s" index="1">iCFG_EN_VEC[15]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_core.vhd" Line 384: Net &lt;<arg fmt="%s" index="1">iCFG_EN_16_0</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_core.vhd" Line 385: Net &lt;<arg fmt="%s" index="1">iCFG_EN_16_1</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\chipscope_ila.vhd" Line 279: Net &lt;<arg fmt="%s" index="1">iCONTROL_IN[17]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\chipscope_ila.vhd" Line 283: Net &lt;<arg fmt="%s" index="1">iATC_CLKIN</arg>&gt; does not have a driver.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\ila_pro_0.vhd</arg>&quot; line <arg fmt="%s" index="2">43</arg>: Output port &lt;<arg fmt="%s" index="3">TRIG_OUT</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DATA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG1</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG2</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG3</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG4</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG5</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG6</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG7</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG8</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG9</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG10</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG11</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG12</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG13</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG14</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG15</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\chipscope_ila.vhd</arg>&quot; line <arg fmt="%s" index="2">1162</arg>: Output port &lt;<arg fmt="%s" index="3">TRIG_OUT</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">I_NO_D.U_ILA</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">iCONTROL_IN&lt;17:15&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">TRIG_OUT</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">iATC_CLKIN</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CONTROL_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CONTROL_IN&lt;2:2&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CONTROL_IN&lt;10:9&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CONTROL_IN&lt;17:14&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CONTROL_IN&lt;34:20&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ATC_CLKIN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_core.vhd</arg>&quot; line <arg fmt="%s" index="2">601</arg>: Output port &lt;<arg fmt="%s" index="3">HALT</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U_RST</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_core.vhd</arg>&quot; line <arg fmt="%s" index="2">627</arg>: Output port &lt;<arg fmt="%s" index="3">CFG_TSEQ_DOUT</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U_TRIG</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_core.vhd</arg>&quot; line <arg fmt="%s" index="2">790</arg>: Output port &lt;<arg fmt="%s" index="3">CAP_EXT_TRIGOUT</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U_G2_SQ.U_CAPCTRL</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_core.vhd</arg>&quot; line <arg fmt="%s" index="2">874</arg>: Output port &lt;<arg fmt="%s" index="3">WR_TSTAMP_OVERFLOW</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U_CAPSTOR</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">iCFG_EN_VEC</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">iCFG_EN_16_0</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">iCFG_EN_16_1</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_trigger.vhd</arg>&quot; line <arg fmt="%s" index="2">254</arg>: Output port &lt;<arg fmt="%s" index="3">CFG_DOUT</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U_TC</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CFG_EN_VEC</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIG_RESET</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CFG_EN_16_0</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CFG_EN_16_1</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_match_combo.vhd</arg>&quot; line <arg fmt="%s" index="2">160</arg>: Output port &lt;<arg fmt="%s" index="3">CFG_DOUT</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U_MU</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">I_MUT_VARX.MODE_Q</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">MODE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">iCFG_EN_VEC</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CFG_EN_VEC</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CAP_ENDSTATE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TSTAMP_IN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CFG_EN_16_0</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CFG_EN_16_1</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_ila_v1_05_a\ila_cap_ctrl_g2_sq.vhd</arg>&quot; line <arg fmt="%s" index="2">468</arg>: Output port &lt;<arg fmt="%s" index="3">CFG_DOUT</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">I_SRLT_NE_1.U_WHCMPCE</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">TRIGGER</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">REWIND</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CLK_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">RESET_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CFG_EN_VEC</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CFG_EN_VEC</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CLK</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">RESET</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CFG_EN_VEC</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CFG_EN_VEC</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CLK</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">RESET</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WR_TSTAMP</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WR_GAP</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WR_REWIND</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">RD_TSTAMP_EN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WR_RESET_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_lib_v1_03_a\cs_bram_simple_s6_ramb9.vhd</arg>&quot; line <arg fmt="%s" index="2">374</arg>: Output port &lt;<arg fmt="%s" index="3">DOBDO</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U_RAMB9</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_lib_v1_03_a\cs_bram_simple_s6_ramb9.vhd</arg>&quot; line <arg fmt="%s" index="2">374</arg>: Output port &lt;<arg fmt="%s" index="3">DOPADOP</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U_RAMB9</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">E:\WorkSpace\Project\Demo_Board\Espier_III_Xilinx\logic\0-example_test_board_x\_ngo\cs_ila_pro_0\tmp\_cg\_bbx\chipscope_lib_v1_03_a\cs_bram_simple_s6_ramb9.vhd</arg>&quot; line <arg fmt="%s" index="2">374</arg>: Output port &lt;<arg fmt="%s" index="3">DOPBDOP</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U_RAMB9</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="2169" delta="new" >HDL ADVISOR - Some clock signals were not automatically buffered by XST with BUFG/BUFR resources. Please use the buffer_type constraint in order to insert these buffers to the clock signals to help prevent skew problems.
</msg>

</messages>

