<?xml version="1.0" encoding="UTF-8"?>
<!-- IMPORTANT: This is an internal file that has been generated
     by the Xilinx ISE software.  Any direct editing or
     changes made to this file may result in unpredictable
     behavior or data corruption.  It is strongly advised that
     users do not edit the contents of this file. -->
<messages>
<msg type="info" file="Xst" num="3231" delta="new" >The small RAM &lt;<arg fmt="%s" index="1">Mram_PWR_1_o_PWR_1_o_mux_17_OUT</arg>&gt; will be implemented on LUTs in order to maximize performance and save block RAM resources. If you want to force its implementation on block, use option/constraint ram_style.
</msg>

<msg type="info" file="Xst" num="2169" delta="new" >HDL ADVISOR - Some clock signals were not automatically buffered by XST with BUFG/BUFR resources. Please use the buffer_type constraint in order to insert these buffers to the clock signals to help prevent skew problems.
</msg>

</messages>

